


**XMOS firmware upgrade instructions**

1. Plug the device into the power supply and USB cable, turn it on, switch to the USB channel, and then open the USB upgrade program according to the figure below.



2. Find the upgrade file in the folder and load it.  
  
  
3. Click “start” to start the upgrade.  
4. After the upgrade, click exit power on the device again.  
